Used by the debugger.
hex representation of a byte.
hex representation of a short.
hex representation of a long.
Disassembled line output.

A simple record to hold breakpoint information it may be completed later with pass count, etc. They must be in a sorted linked list.

A record to store line number information and a list of breakpoints.
Generate Line Number information specific to a given range.
Discard Line Number Information.
Toggle a breakpoint.
Set a breakpoint on a given address.
Clear one specific breakpoint.
Clear the breakpoint list.
Find one breakpoint at a given address.
Returns the current disassembled line at Code(IP).
Returns the length of the current opcode at Code(IP).
Returns a 8-bit hexadecimal string.
Returns a 16-bit hexadecimal string.
Returns a 32-bit hexadecimal string.